**Truck Wash Procedure**

When a truck arrives at the facility to be cleaned, it is backed into the secondary containment. It is connected to a hydro vac truck using a 4 inch hose. All of the materials are transfered from the truck being cleaned to the hydro vac via the 4 inch hose. Once the truck(s) are cleaned, the hydro vac takes the material directly to a landfill / disposal site. The material is never transferred to a third truck or to a storage tank. The secondary containment is used as a spill prevention method. The containment is in place to catch a spill in case a valve would begin to leak or a hose would erupt.